Touch Driver for Windows 2000/XP/Vista/7/8/8.1/10/11

If you are running Windows 7 or Windows 2008 Server R2, please do the follow the steps below:

Step1. Ensure that the platform is upgraded to at least Service Pack 1

Step2. Install the appropriate Windows KB update for your operating system

Setp3. You can download the KB’s from links below:

https://www.catalog.update.microsoft.com/Search.aspx?q=4474419

;************************************************************
;**               command line touch utility               **
;************************************************************

Open command line touch utility
1. Open the Command Prompt with Administrative Privileges
2. Open touch utility
c:\Program Files\Touch Utility\Setparams.exe

or

Usage: Setparams [options] [command] [value]

options:
D<1, 2...> [command] [value]       (setting by device number)
S<1, 2...> [command] [value]       (setting by screen number)
C<1, 2...> [command] [value]       (setting by COM port number)
ALL [command] [value]              (setting all touch devices)
--path="<location path>" [command] [value]       (setting by location path)
--query                            (query device information)
double-click-speed <200~900>       (Mouse Double Click Speed)
double-click-area  <10~60>         (Mouse Double Click Area)
multi-monitor-mode <0: Auto 1: Resolution Mode 2: Offset mode>  (Multi Monitor Mode)

Commands and values(projected capacitive touch screen):
-b, --beep <disable,down,up,down-and-up>                    (Beep On)
-p, --play <disable,buzzer,media>                           (Play Method)
-f, --freq <500~3000>                                       (Sound Frequency)
-e, --dura <20~50>                                          (Sound Duration)
-h, --hid  <digitizer,mouse>                                (HID Mode)
-s, --screen <1~n>                                          (Map Screen Number)
-c, --touch-mode <mouseemu,click-on-touch,click-on-release> (Mouse Click Mode)
-r, --right-click <enable,disable>                          (Mouse Auto Right-Click)
-a, --right-click-time <1~15>                               (Mouse Auto Right-Click Time)

Commands and values(resistive touch screen):
-b, --beep <disable,down,up,down-and-up>   (Beep ON)
-p, --play <disable,buzzer,media>          (play method)
-f, --freq <500~3000>                      (Sound Frequency)
-e, --dura <20~50>                         (Sound Duration)
-h, --hid  <digitizer,mouse>               (HID Mode)
-i, --auto-set-hid <enable,disable>        (auto set HID mode to digitizer)
-c, --report-mode <drawing,button>         (Mouse Report Mode)
-r, --right-click <enable,disable>         (Mouse Auto Right-Click)
-a, --right-click-time <1~15>              (Mouse Auto Right-Click Time)
-t, --disable-report <enable,disable>      (disable report)
-s, --screen <1~n>                         (Map Screen Number)
-k, --first-move <enable,disable>          (First Move)
-g, --edge-right <0~500>                   (Edge Compensation of Right)
-l, --edge-left <0~500>                    (Edge Compensation of Left)
-q, --edge-bottom <0~500>                  (Edge Compensation of Bottom)
-u, --edge-up <0~500>                      (Edge Compensation of Up)

example:

Set all device to digitizer

c:\Program Files\Touch Utility\Setparams.exe ALL -h digitizer

or

c:\Program Files\Touch Utility\Setparams.exe ALL --hid digitizer

;************************************************************
Set device 1 to digitizer

c:\Program Files\Touch Utility\Setparams.exe D1 -h digitizer

or

c:\Program Files\Touch Utility\Setparams.exe D1 --hid digitizer

;************************************************************
Set screen 1 to digitizer

c:\Program Files\Touch Utility\Setparams.exe S1 -h digitizer

or

c:\Program Files\Touch Utility\Setparams.exe S1 --hid digitizer

;************************************************************
;**                  Resistive touch screen                **
;************************************************************

***********************Usage: **********************************
** DisableReport Dx n
** D=Device Number
** x=1, 2...
** n=0:Enable Report 1:Disable Report

** DisableReport Sx n
** D=Screen Number
** x=1, 2...
** n=0:Enable Report 1:Disable Report

** DisableReport Cx n
** C=COM Port Number
** x=1, 2...
** n=0:Enable Report 1:Disable Report

** DisableReport --path="<Location path>" n
** path=Location path
** n=0:Enable Report 1:Disable Report

** DisableReport --query
** --query     get available devices information
****************************************************************
example1: 
disable device 1
c:\Program Files\Touch Utility\DisableReport.exe D1 1

enbale device 1
c:\Program Files\Touch Utility\DisableReport.exe D1 0

example2:
disable screen 1
c:\Program Files\Touch Utility\DisableReport.exe S1 1

enable screen 1
c:\Program Files\Touch Utility\DisableReport.exe S1 0

example3:
disable COM1
c:\Program Files\Touch Utility\DisableReport.exe C1 1

enable COM1
c:\Program Files\Touch Utility\DisableReport.exe C1 0

example4:
disable report by Location path.
DisableReport --path="SERPANEL4" 1

enable report by Location path.
DisableReport --path="SERPANEL4" 0

example5:
get location path.
c:\Program Files\Touch Utility\DisableReport --query

;************************************************************
;**                      Silent instaall                   **
;************************************************************
xxx_Setup_x.x.x.x.exe /VERYSILENT /NORESTART /NOCANCEL /SUPPRESSMSGBOXES /SP-
